SAE 2263 Data Analysis
Report Generated on Feb 16 2026 at 12:53:16 
Program Version 1.3.1

Test Date:              
Vehicle Config Number:  
License Number:         

Area:                   20.56 Ft^2
Weight:                 3257.55 lbs
Corrected Weight:       3257.55 lbs
Inertia Weight:         3257.55 lbs

Pressure:               29.92 inHg
Temperature:            77 F

Test Range
From 10 MPH to 70 MPH

Average Wind
Head: 0.05 Cross: 0.65
Max Wind
Head: 1.61 Cross: 1.41

Mechanical terms corrected to standard temperature of  20 C
Aero terms corrected to standard pressure of  98.21 kPa

TIRE INFORMATION
   ID#     Tire Size      Manuf   Tire Name      Pressure
RF                                               
LF                                               
RR                                               
LR                                               

CALIBRATION COEFFICIENTS
Nash Calibrator

Ka =  0.9928 
k3 = -0.000004
K4 =  0.134112 

Ky = 1.010593
Yaw Offset = 0.521000

SOLVER INFORMATION
Regression Solver

 3 term mechanical model
 5 term aerodynamic model

RESULTS
Amech: 30.04 lbs
Bmech: 0.0766 lbs/MPH
Cmech: 0.002862 lbs/MPH ^ 2

Caero: 0.018807 lbs/MPH ^ 2
Ctotl: 0.021669 lbs/MPH ^ 2

Area:  20.56 Ft^2
Cd:    0.376

COMMENTS

